De Havilland DHC-5 Buffalo
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 49,201 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed @ FL170 | 242 KIAS
VMO - Maximum Operating Speed @ FL200 | 232 KIAS
VMO - Maximum Operating Speed @ FL250 | 214 KIAS
MMO - Maximum Operating Speed Mach | .50 Mach
Turbulent Air Penetration Speed | 190 KIAS
VA - Maneuvering Speed | 177 KIAS
VMC - Minimum Control Speed | 103 KIAS
VX - Two-engine Best Angle-of-Climb | 135 KIAS
VY - Two-engine Best Rate of Climb | 145 KIAS
Best Glide Speed both engines inoperative | 135 KIAS

VFE - Maximum Flaps Extended Speed

Flaps | KIAS
Flaps 5 | 163
Flap 10 | 154
Flap 15 | 150
Flap 35 | 138

V1 - Takeoff Decision Speed dry runwayStandard temperature, 500 ft pressure altitude
Standard temperature, 500 ft pressure altitude

49,000 lbs | 142 KIAS
<38,000 lbs | 132 KIAS

VR - Rotation Speed dry runway - flaps 15
Standard temperature, 500 ft pressure altitude

37 49,000 lbs | 145 KIAS
<28,000 lbs | 135 KIAS

V2 - Takeoff Safety Speed dry runway - flaps 15
Standard temperature, 500 ft pressure altitude

37,000 lbs | 148 KIAS
<28,000 lbs | 142 KIAS

VREF - Landing Approach Speed - flaps 35 - gear down

37,000 lbs | 144 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

    Quick Reference - EYEPOINT KEY COMMANDS

    Move Eyepoint Back

    CTRL+ENTER

    Move Eyepoint Down

    SHIFT+BACKSPACE

    Move Eyepoint Forward

    CTRL+BACKSPACE

    Move Eyepoint Left

    CTRL+SHIFT+BACKSPACE

    Move Eyepoint Right

    CTRL+SHIFT+ENTER

    Move Eyepoint Up

    SHIFT+ENTER

    Reset Eyepoint

    SPACE

Copyright 2008 - Premier Aircraft Design